VERSION 6
BEGIN SCHEMATIC
    BEGIN ATTR DeviceFamilyName "spartan2e"
        DELETE all:0
        EDITNAME all:0
        EDITTRAIT all:0
    END ATTR
    BEGIN NETLIST
        SIGNAL "Din(15:0)"
        SIGNAL "Write"
        SIGNAL "clk"
        SIGNAL "out(15:0)"
        SIGNAL "out(3:0)"
        SIGNAL "out(15:12)"
        SIGNAL "out(11:8)"
        SIGNAL "out(7:4)"
        PORT Input "Din(15:0)"
        PORT Input "Write"
        PORT Input "clk"
        PORT Output "out(3:0)"
        PORT Output "out(15:12)"
        PORT Output "out(11:8)"
        PORT Output "out(7:4)"
        BEGIN BLOCKDEF "instructionreg"
            TIMESTAMP 2003 11 12 22 0 21
            RECTANGLE N 32 0 448 176 
            BEGIN LINE W 0 48 32 48 
            END LINE
            LINE N 0 80 32 80 
            LINE N 0 112 32 112 
            BEGIN LINE W 448 48 480 48 
            END LINE
            BEGIN LINE W 448 48 480 48 
            END LINE
        END BLOCKDEF
        BEGIN BLOCK "XLXI_1" "instructionreg"
            PIN "D(15:0)" "Din(15:0)"
            PIN "CE" "Write"
            PIN "CLK" "clk"
            PIN "Q(15:0)" "out(15:0)"
        END BLOCK
    END NETLIST
    BEGIN SHEET 1 3520 2720
        BEGIN INSTANCE "XLXI_1" 1392 1136 R0
        END INSTANCE
        BEGIN BRANCH "Din(15:0)"
            WIRE 1200 944 1376 944
            WIRE 1376 944 1376 1184
            WIRE 1376 1184 1392 1184
        END BRANCH
        BEGIN BRANCH "Write"
            WIRE 1120 1216 1376 1216
            WIRE 1376 1216 1392 1216
        END BRANCH
        BEGIN BRANCH "clk"
            WIRE 1120 1392 1376 1392
            WIRE 1376 1248 1392 1248
            WIRE 1376 1248 1376 1392
        END BRANCH
        IOMARKER 1200 944 "Din(15:0)" R180 28
        IOMARKER 1120 1216 "Write" R180 28
        IOMARKER 1120 1392 "clk" R180 28
        BEGIN BRANCH "out(15:0)"
            WIRE 1872 1184 2112 1184
            BEGIN DISPLAY 2112 1184 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "out(15:12)"
            WIRE 1776 1536 2176 1536
        END BRANCH
        BEGIN BRANCH "out(11:8)"
            WIRE 1776 1632 2176 1632
        END BRANCH
        BEGIN BRANCH "out(7:4)"
            WIRE 1776 1728 2176 1728
        END BRANCH
        BEGIN BRANCH "out(3:0)"
            WIRE 1776 1824 2176 1824
        END BRANCH
        IOMARKER 2176 1536 "out(15:12)" R0 28
        IOMARKER 2176 1632 "out(11:8)" R0 28
        IOMARKER 2176 1728 "out(7:4)" R0 28
        IOMARKER 2176 1824 "out(3:0)" R0 28
    END SHEET
END SCHEMATIC
