VERSION 6
BEGIN SCHEMATIC
    BEGIN ATTR DeviceFamilyName "spartan2e"
        DELETE all:0
        EDITNAME all:0
        EDITTRAIT all:0
    END ATTR
    BEGIN NETLIST
        SIGNAL "REGWRITE"
        SIGNAL "IR(12)"
        SIGNAL "IR(13)"
        SIGNAL "IR(14)"
        SIGNAL "IR(15)"
        SIGNAL "INTERRUPT"
        SIGNAL "IR(0)"
        SIGNAL "IR(1)"
        SIGNAL "IR(2)"
        SIGNAL "IR(3)"
        SIGNAL "RESET"
        SIGNAL "ZCValue"
        SIGNAL "IR(0:15)"
        SIGNAL "IRWrite"
        SIGNAL "MemWrite"
        SIGNAL "PCWrite"
        SIGNAL "Mux0"
        SIGNAL "Mux1(0:2)"
        SIGNAL "Mux2"
        SIGNAL "Mux5"
        SIGNAL "Mux6(0:2)"
        SIGNAL "Mux7(0:2)"
        SIGNAL "Mux8(0:1)"
        SIGNAL "Mux9"
        SIGNAL "Mux10"
        SIGNAL "ALUOp(0:2)"
        SIGNAL "ALUOp(0)"
        SIGNAL "ALUOp(1)"
        SIGNAL "ALUOp(2)"
        SIGNAL "SPCWrite(1)"
        SIGNAL "Mux1(0)"
        SIGNAL "Mux1(1)"
        SIGNAL "Mux1(2)"
        SIGNAL "Mux6(0)"
        SIGNAL "Mux6(1)"
        SIGNAL "Mux7(0)"
        SIGNAL "Mux7(1)"
        SIGNAL "Mux7(2)"
        SIGNAL "Mux8(0)"
        SIGNAL "Mux8(1)"
        SIGNAL "SPCWrite(0)"
        SIGNAL "SPCWrite(0:3)"
        SIGNAL "SPCWrite(2)"
        SIGNAL "SPCWrite(3)"
        SIGNAL "Mux3(0:1)"
        SIGNAL "Mux3(0)"
        SIGNAL "Mux3(1)"
        SIGNAL "Mux6(2)"
        SIGNAL "CLK"
        SIGNAL "XLXN_4"
        SIGNAL "IR(4)"
        SIGNAL "IR(5)"
        SIGNAL "IR(6)"
        SIGNAL "IR(7)"
        SIGNAL "IR(8)"
        SIGNAL "IR(9)"
        SIGNAL "IR(10)"
        SIGNAL "IR(11)"
        SIGNAL "XLXN_13"
        SIGNAL "XLXN_14"
        SIGNAL "XLXN_15"
        SIGNAL "XLXN_16"
        SIGNAL "XLXN_17"
        SIGNAL "XLXN_18"
        SIGNAL "XLXN_19"
        SIGNAL "XLXN_30"
        SIGNAL "XLXN_31"
        SIGNAL "XLXN_32"
        PORT Output "REGWRITE"
        PORT Input "INTERRUPT"
        PORT Input "RESET"
        PORT Input "ZCValue"
        PORT Input "IR(0:15)"
        PORT Output "IRWrite"
        PORT Output "MemWrite"
        PORT Output "PCWrite"
        PORT Output "Mux0"
        PORT Output "Mux1(0:2)"
        PORT Output "Mux2"
        PORT Output "Mux5"
        PORT Output "Mux6(0:2)"
        PORT Output "Mux7(0:2)"
        PORT Output "Mux8(0:1)"
        PORT Output "Mux9"
        PORT Output "Mux10"
        PORT Output "ALUOp(0:2)"
        PORT Output "SPCWrite(0:3)"
        PORT Output "Mux3(0:1)"
        BEGIN BLOCKDEF "constate"
            TIMESTAMP 2003 11 1 0 58 36
            LINE N 368 1696 432 1696 
            LINE N 368 1760 432 1760 
            LINE N 368 1952 432 1952 
            LINE N 368 1568 432 1568 
            LINE N 368 1632 432 1632 
            LINE N 368 32 432 32 
            LINE N 368 96 432 96 
            LINE N 368 160 432 160 
            LINE N 368 224 432 224 
            LINE N 368 288 432 288 
            LINE N 368 352 432 352 
            LINE N 368 416 432 416 
            LINE N 368 480 432 480 
            LINE N 368 544 432 544 
            LINE N 368 608 432 608 
            LINE N 368 672 432 672 
            LINE N 368 800 432 800 
            LINE N 368 864 432 864 
            LINE N 368 928 432 928 
            LINE N 368 992 432 992 
            LINE N 368 1056 432 1056 
            LINE N 368 1120 432 1120 
            LINE N 368 1184 432 1184 
            LINE N 368 1248 432 1248 
            LINE N 368 1312 432 1312 
            LINE N 368 1376 432 1376 
            LINE N 368 1440 432 1440 
            LINE N 368 1504 432 1504 
            LINE N 64 -736 0 -736 
            LINE N 64 -672 0 -672 
            LINE N 64 -608 0 -608 
            LINE N 64 -544 0 -544 
            LINE N 64 -480 0 -480 
            LINE N 64 -416 0 -416 
            LINE N 64 -352 0 -352 
            LINE N 64 -288 0 -288 
            LINE N 64 -224 0 -224 
            LINE N 64 -160 0 -160 
            LINE N 64 -96 0 -96 
            LINE N 64 -32 0 -32 
            LINE N 368 -736 432 -736 
            RECTANGLE N 64 -768 368 1984 
        END BLOCKDEF
        BEGIN BLOCKDEF "and12"
            TIMESTAMP 2001 2 2 12 53 52
            LINE N 256 -416 192 -416 
            LINE N 144 -368 64 -368 
            LINE N 64 -464 144 -464 
            ARC N 96 -464 192 -368 144 -368 144 -464 
            LINE N 0 -704 64 -704 
            LINE N 0 -512 64 -512 
            LINE N 0 -448 64 -448 
            LINE N 0 -384 64 -384 
            LINE N 0 -320 64 -320 
            LINE N 0 -256 64 -256 
            LINE N 0 -192 64 -192 
            LINE N 0 -128 64 -128 
            LINE N 0 -64 64 -64 
            LINE N 0 -576 64 -576 
            LINE N 0 -640 64 -640 
            LINE N 0 -768 64 -768 
            LINE N 64 -768 64 -64 
        END BLOCKDEF
        BEGIN BLOCK "XLXI_1" "constate"
            PIN "CLK" "CLK"
            PIN "FUNCT0" "IR(12)"
            PIN "FUNCT1" "IR(13)"
            PIN "FUNCT2" "IR(14)"
            PIN "FUNCT3" "IR(15)"
            PIN "INTERRUPT" "INTERRUPT"
            PIN "OPCODE0" "IR(0)"
            PIN "OPCODE1" "IR(1)"
            PIN "OPCODE2" "IR(2)"
            PIN "OPCODE3" "IR(3)"
            PIN "RESET" "RESET"
            PIN "ZCValue" "ZCValue"
            PIN "ALUOp0" "ALUOp(0)"
            PIN "ALUOp1" "ALUOp(1)"
            PIN "ALUOp2" "ALUOp(2)"
            PIN "EPCWRITE" "SPCWrite(1)"
            PIN "INTWRITE" "SPCWrite(2)"
            PIN "IRWRITE" "IRWrite"
            PIN "MEMWRITE" "MemWrite"
            PIN "Mux0" "Mux0"
            PIN "Mux1b0" "Mux1(0)"
            PIN "Mux1b1" "Mux1(1)"
            PIN "Mux1b2" "Mux1(2)"
            PIN "Mux2" "Mux2"
            PIN "Mux3b0" "Mux3(0)"
            PIN "Mux3b1" "Mux3(1)"
            PIN "Mux5" "Mux5"
            PIN "Mux6b0" "Mux6(0)"
            PIN "Mux6b1" "Mux6(1)"
            PIN "Mux6b2" "Mux6(2)"
            PIN "Mux7b0" "Mux7(0)"
            PIN "Mux7b1" "Mux7(1)"
            PIN "Mux7b2" "Mux7(2)"
            PIN "Mux8b0" "Mux8(0)"
            PIN "Mux8b1" "Mux8(1)"
            PIN "Mux9" "Mux9"
            PIN "Mux10" "Mux10"
            PIN "OUTWRITE" "SPCWrite(3)"
            PIN "PCWRITE" "PCWrite"
            PIN "REGWRITE" "REGWRITE"
            PIN "SPECIALWRITE" "SPCWrite(0)"
        END BLOCK
        BEGIN BLOCK "XLXI_4" "and12"
            PIN "I0" "XLXN_32"
            PIN "I1" "XLXN_32"
            PIN "I10" "IR(5)"
            PIN "I11" "IR(4)"
            PIN "I2" "XLXN_32"
            PIN "I3" "XLXN_32"
            PIN "I4" "IR(11)"
            PIN "I5" "IR(10)"
            PIN "I6" "IR(9)"
            PIN "I7" "IR(8)"
            PIN "I8" "IR(7)"
            PIN "I9" "IR(6)"
            PIN "O" "XLXN_32"
        END BLOCK
    END NETLIST
    BEGIN SHEET 1 5440 3520
        BEGIN BRANCH "REGWRITE"
            WIRE 1824 144 1984 144
        END BRANCH
        BEGIN BRANCH "IR(12)"
            WIRE 1104 208 1392 208
            BEGIN DISPLAY 1104 208 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IR(13)"
            WIRE 1088 272 1392 272
            BEGIN DISPLAY 1088 272 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IR(14)"
            WIRE 1120 336 1392 336
            BEGIN DISPLAY 1120 336 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IR(15)"
            WIRE 1120 400 1392 400
            BEGIN DISPLAY 1120 400 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "INTERRUPT"
            WIRE 1104 464 1392 464
            BEGIN DISPLAY 1104 464 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IR(0)"
            WIRE 1104 528 1392 528
            BEGIN DISPLAY 1104 528 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IR(1)"
            WIRE 1104 592 1392 592
            BEGIN DISPLAY 1104 592 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IR(2)"
            WIRE 1120 656 1392 656
            BEGIN DISPLAY 1120 656 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IR(3)"
            WIRE 1104 720 1392 720
            BEGIN DISPLAY 1104 720 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "RESET"
            WIRE 1104 784 1392 784
            BEGIN DISPLAY 1104 784 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "ZCValue"
            WIRE 1104 848 1392 848
            BEGIN DISPLAY 1104 848 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IR(0:15)"
            WIRE 272 688 496 688
            BEGIN DISPLAY 496 688 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "INTERRUPT"
            WIRE 272 608 512 608
            BEGIN DISPLAY 512 608 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "RESET"
            WIRE 304 800 480 800
            BEGIN DISPLAY 480 800 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "ZCValue"
            WIRE 304 912 496 912
            BEGIN DISPLAY 496 912 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IRWrite"
            WIRE 2784 832 3168 832
            BEGIN DISPLAY 2784 832 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "MemWrite"
            WIRE 2784 976 3200 976
            BEGIN DISPLAY 2784 976 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "PCWrite"
            WIRE 2784 1152 3200 1152
            BEGIN DISPLAY 2784 1152 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux0"
            WIRE 2784 1520 3184 1520
            BEGIN DISPLAY 2784 1520 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux1(0:2)"
            WIRE 2784 1648 3168 1648
            BEGIN DISPLAY 2784 1648 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux2"
            WIRE 2800 1760 3152 1760
            BEGIN DISPLAY 2800 1760 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux5"
            WIRE 2768 1968 3168 1968
            BEGIN DISPLAY 2768 1968 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux6(0:2)"
            WIRE 2768 2080 3168 2080
            BEGIN DISPLAY 2768 2080 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux7(0:2)"
            WIRE 2752 2192 3168 2192
            BEGIN DISPLAY 2752 2192 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux8(0:1)"
            WIRE 2736 2304 3200 2304
            BEGIN DISPLAY 2736 2304 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux9"
            WIRE 2784 2416 3120 2416
            BEGIN DISPLAY 2784 2416 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux10"
            WIRE 2832 2544 3168 2544
            BEGIN DISPLAY 2832 2544 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "ALUOp(0:2)"
            WIRE 2768 544 3168 544
            BEGIN DISPLAY 2768 544 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "ALUOp(0)"
            WIRE 1824 912 1920 912
            BEGIN DISPLAY 1920 912 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "ALUOp(1)"
            WIRE 1824 976 1936 976
            BEGIN DISPLAY 1936 976 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "ALUOp(2)"
            WIRE 1824 1040 1920 1040
            BEGIN DISPLAY 1920 1040 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "SPCWrite(1)"
            WIRE 1824 1104 1904 1104
            BEGIN DISPLAY 1904 1104 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IRWrite"
            WIRE 1824 1168 1904 1168
            BEGIN DISPLAY 1904 1168 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "MemWrite"
            WIRE 1824 1232 1920 1232
            BEGIN DISPLAY 1920 1232 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux0"
            WIRE 1824 1296 1920 1296
            BEGIN DISPLAY 1920 1296 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux1(0)"
            WIRE 1824 1360 1904 1360
            BEGIN DISPLAY 1904 1360 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux1(1)"
            WIRE 1824 1424 1904 1424
            BEGIN DISPLAY 1904 1424 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux1(2)"
            WIRE 1824 1488 1904 1488
            BEGIN DISPLAY 1904 1488 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux2"
            WIRE 1824 1552 1904 1552
            BEGIN DISPLAY 1904 1552 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux5"
            WIRE 1824 1680 1904 1680
            BEGIN DISPLAY 1904 1680 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux6(0)"
            WIRE 1824 1744 1904 1744
            BEGIN DISPLAY 1904 1744 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux6(1)"
            WIRE 1824 1808 1904 1808
            BEGIN DISPLAY 1904 1808 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux7(0)"
            WIRE 1824 1872 1904 1872
            BEGIN DISPLAY 1904 1872 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux7(1)"
            WIRE 1824 1936 1888 1936
            BEGIN DISPLAY 1888 1936 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux7(2)"
            WIRE 1824 2000 1888 2000
            BEGIN DISPLAY 1888 2000 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux8(0)"
            WIRE 1824 2064 1904 2064
            BEGIN DISPLAY 1904 2064 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux8(1)"
            WIRE 1824 2128 1872 2128
            BEGIN DISPLAY 1872 2128 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux9"
            WIRE 1824 2192 1888 2192
            BEGIN DISPLAY 1888 2192 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux10"
            WIRE 1824 2256 1904 2256
            BEGIN DISPLAY 1904 2256 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "PCWrite"
            WIRE 1824 2320 1888 2320
            BEGIN DISPLAY 1888 2320 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "SPCWrite(0)"
            WIRE 1824 2384 1872 2384
            BEGIN DISPLAY 1872 2384 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "SPCWrite(0:3)"
            WIRE 2736 672 3152 672
            BEGIN DISPLAY 2736 672 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "SPCWrite(2)"
            WIRE 1824 2448 1952 2448
            BEGIN DISPLAY 1952 2448 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "SPCWrite(3)"
            WIRE 1824 2512 1936 2512
            BEGIN DISPLAY 1936 2512 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        IOMARKER 272 688 "IR(0:15)" R180 28
        IOMARKER 272 608 "INTERRUPT" R180 28
        IOMARKER 304 800 "RESET" R180 28
        IOMARKER 304 912 "ZCValue" R180 28
        IOMARKER 1984 144 "REGWRITE" R0 28
        IOMARKER 3168 544 "ALUOp(0:2)" R0 28
        IOMARKER 3168 832 "IRWrite" R0 28
        IOMARKER 3200 976 "MemWrite" R0 28
        IOMARKER 3200 1152 "PCWrite" R0 28
        IOMARKER 3184 1520 "Mux0" R0 28
        IOMARKER 3168 1648 "Mux1(0:2)" R0 28
        IOMARKER 3152 1760 "Mux2" R0 28
        IOMARKER 3168 1968 "Mux5" R0 28
        IOMARKER 3168 2080 "Mux6(0:2)" R0 28
        IOMARKER 3168 2192 "Mux7(0:2)" R0 28
        IOMARKER 3200 2304 "Mux8(0:1)" R0 28
        IOMARKER 3120 2416 "Mux9" R0 28
        IOMARKER 3168 2544 "Mux10" R0 28
        IOMARKER 3152 672 "SPCWrite(0:3)" R0 28
        BEGIN BRANCH "Mux3(0:1)"
            WIRE 2800 1872 3168 1872
            BEGIN DISPLAY 2800 1872 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        IOMARKER 3168 1872 "Mux3(0:1)" R0 28
        BEGIN BRANCH "Mux3(0)"
            WIRE 1824 2576 1984 2576
            BEGIN DISPLAY 1984 2576 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Mux3(1)"
            WIRE 1824 2640 1968 2640
            BEGIN DISPLAY 1968 2640 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN INSTANCE "XLXI_1" 1392 880 R0
        END INSTANCE
        BEGIN BRANCH "Mux6(2)"
            WIRE 1824 2832 1952 2832
            BEGIN DISPLAY 1952 2832 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "CLK"
            WIRE 976 144 1392 144
            BEGIN DISPLAY 976 144 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IR(11)"
            WIRE 800 1616 816 1616
            WIRE 816 1616 960 1616
            WIRE 960 1616 960 1632
            WIRE 960 1632 1072 1632
            BEGIN DISPLAY 800 1616 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IR(10)"
            WIRE 816 1552 832 1552
            WIRE 832 1552 928 1552
            WIRE 928 1552 928 1568
            WIRE 928 1568 1072 1568
            BEGIN DISPLAY 816 1552 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IR(9)"
            WIRE 816 1488 832 1488
            WIRE 832 1488 944 1488
            WIRE 944 1488 944 1504
            WIRE 944 1504 1072 1504
            BEGIN DISPLAY 816 1488 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IR(8)"
            WIRE 784 1440 800 1440
            WIRE 800 1440 928 1440
            WIRE 928 1440 1072 1440
            BEGIN DISPLAY 784 1440 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IR(7)"
            WIRE 800 1392 816 1392
            WIRE 816 1392 944 1392
            WIRE 944 1376 944 1392
            WIRE 944 1376 1072 1376
            BEGIN DISPLAY 800 1392 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IR(6)"
            WIRE 800 1328 816 1328
            WIRE 816 1328 960 1328
            WIRE 960 1312 960 1328
            WIRE 960 1312 1072 1312
            BEGIN DISPLAY 800 1328 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IR(5)"
            WIRE 800 1264 816 1264
            WIRE 816 1264 960 1264
            WIRE 960 1248 960 1264
            WIRE 960 1248 1072 1248
            BEGIN DISPLAY 800 1264 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "IR(4)"
            WIRE 800 1184 816 1184
            WIRE 816 1184 976 1184
            WIRE 976 1184 1072 1184
            BEGIN DISPLAY 800 1184 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        INSTANCE "XLXI_4" 1072 1952 R0
        BEGIN BRANCH "XLXN_32"
            WIRE 864 1696 1072 1696
            WIRE 864 1696 864 1760
            WIRE 864 1760 864 1776
            WIRE 864 1776 864 1824
            WIRE 864 1824 864 1824
            WIRE 864 1824 864 1888
            WIRE 864 1888 864 1984
            WIRE 864 1984 1328 1984
            WIRE 864 1888 1072 1888
            WIRE 864 1824 1072 1824
            WIRE 864 1760 1072 1760
            WIRE 1328 1536 1344 1536
            WIRE 1344 1536 1344 1968
            WIRE 1328 1968 1344 1968
            WIRE 1328 1968 1328 1984
        END BRANCH
    END SHEET
END SCHEMATIC
