
**** 03/25/04 17:14:17 ******* PSpice 10.0.0 (Jan 2003) ******* ID# 1111111111 
 ** Profile: "SCHEMATIC1-test"  [ C:\docume~1\LAFLEN\DESKTOP\ece130Cadence\CadenceClassExample-PSpiceFiles\SCHEMATIC1\test.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "test.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.STMLIB "../../../cadenceclassexample-pspicefiles/cadenceclassexample.stl" 
* From [PSPICE NETLIST] section of C:\Cadence\PSD_15.0\tools\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 1000ns 0 
.PROBE V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source CADENCECLASSEXAMPLE
X_U6         A_ B_ C_ Z $G_DPWR $G_DGND OR3
U_B         STIM(1,0) $G_DPWR $G_DGND B IO_STM STIMULUS=B
X_U1A         X Y Z F $G_DPWR $G_DGND 7411 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0
X_U7         A A_  $G_DPWR $G_DGND INV
X_U3A         X2 Y2 Z2 F2 $G_DPWR $G_DGND 7427 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0
U_C         STIM(1,0) $G_DPWR $G_DGND C IO_STM STIMULUS=C
X_U3B         A_ B_ C_ Z2 $G_DPWR $G_DGND 7427 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0
X_U4A         A B Y2 $G_DPWR $G_DGND 7428 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0
X_U8         B B_  $G_DPWR $G_DGND INV
X_U4B         A C X2 $G_DPWR $G_DGND 7428 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0
X_U5A         A C X $G_DPWR $G_DGND 7432 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0
X_U9         C C_  $G_DPWR $G_DGND INV
X_U5B         A B Y $G_DPWR $G_DGND 7432 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0
U_A         STIM(1,0) $G_DPWR $G_DGND A IO_STM STIMULUS=A

**** RESUMING test.cir ****
.END

* C:\docume~1\LAFLEN\DESKTOP\ece130Cadence\CadenceClassExample-PSpiceFiles\cadenceclassexample.stl written on Thu Mar 25 17:11:43 20
* by Stimulus Editor -- Serial Number: 1111111111 -- Version 10.0.0
;!Stimulus Get
;! A Digital B Digital C Digital
;!Ok
;!Plot Axis_Settings
;!Xrange 0s 3.5us
;!AutoUniverse
;!XminRes 1ns
;!YminRes 1n
;!Ok
.STIMULUS A STIM (1, 1) ;! CLOCKP 800n 400n 0 0
+   +0s 0
+   +400ns 1
+   Repeat Forever
+      +400ns 0
+      +400ns 1
+   EndRepeat
.STIMULUS B STIM (1, 1) ;! CLOCKP 400n 200n 0 0
+   +0s 0
+   +200ns 1
+   Repeat Forever
+      +200ns 0
+      +200ns 1
+   EndRepeat
.STIMULUS C STIM (1, 1) ;! CLOCKP 200n 100n 0 0
+   +0s 0
+   +100ns 1
+   Repeat Forever
+      +100ns 0
+      +100ns 1
+   EndRepeat

**** 03/25/04 17:14:17 ******* PSpice 10.0.0 (Jan 2003) ******* ID# 1111111111 
 ** Profile: "SCHEMATIC1-test"  [ C:\docume~1\LAFLEN\DESKTOP\ece130Cadence\CadenceClassExample-PSpiceFiles\SCHEMATIC1\test.sim ] 


 ****     Digital Gate MODEL PARAMETERS


******************************************************************************




               D_PLD_GATE      D_11            D_27            D_28            
      TPLHMN    0               6.750001E-09    4.000000E-09    2.400000E-09 
      TPLHTY    0              16.875000E-09   10.000000E-09    6.000000E-09 
      TPLHMX    0              27.000000E-09   15.000000E-09    9.000000E-09 
      TPHLMN    0               4.750000E-09    2.800000E-09    3.200000E-09 
      TPHLTY    0              11.875000E-09    7.000000E-09    8.000000E-09 
      TPHLMX    0              19.000000E-09   11.000000E-09   12.000000E-09 


               D_32            
      TPLHMN    4.000000E-09 
      TPLHTY   10.000000E-09 
      TPLHMX   15.000000E-09 
      TPHLMN    5.600000E-09 
      TPHLTY   14.000000E-09 
      TPHLMX   22.000000E-09 


**** 03/25/04 17:14:17 ******* PSpice 10.0.0 (Jan 2003) ******* ID# 1111111111 
 ** Profile: "SCHEMATIC1-test"  [ C:\docume~1\LAFLEN\DESKTOP\ece130Cadence\CadenceClassExample-PSpiceFiles\SCHEMATIC1\test.sim ] 


 ****     Digital IO  MODEL PARAMETERS


******************************************************************************




               IO_STM          IO_PLD          IO_STD          
        DRVL    0                             104            
        DRVH    0                              96.4          
       AtoD1                                 AtoD_STD        
       AtoD2                                 AtoD_STD_NX     
       AtoD3                                 AtoD_STD        
       AtoD4                                 AtoD_STD_NX     
       DtoA1 DtoA_STM                        DtoA_STD        
       DtoA2 DtoA_STM                        DtoA_STD        
       DtoA3 DtoA_STM                        DtoA_STD        
       DtoA4 DtoA_STM                        DtoA_STD        
      TSWHL1                                    1.511000E-09 
      TSWHL2                                    1.487000E-09 
      TSWHL3                                    1.511000E-09 
      TSWHL4                                    1.487000E-09 
      TSWLH1                                    3.517000E-09 
      TSWLH2                                    3.564000E-09 
      TSWLH3                                    3.517000E-09 
      TSWLH4                                    3.564000E-09 
       TPWRT  100.000000E+03  100.000000E+03  100.000000E+03 



          JOB CONCLUDED

**** 03/25/04 17:14:17 ******* PSpice 10.0.0 (Jan 2003) ******* ID# 1111111111 
 ** Profile: "SCHEMATIC1-test"  [ C:\docume~1\LAFLEN\DESKTOP\ece130Cadence\CadenceClassExample-PSpiceFiles\SCHEMATIC1\test.sim ] 


 ****     JOB STATISTICS SUMMARY


******************************************************************************



  Total job time                    =         .07
