VERSION 6
BEGIN SCHEMATIC
    BEGIN ATTR DeviceFamilyName "spartan2e"
        DELETE all:0
        EDITNAME all:0
        EDITTRAIT all:0
    END ATTR
    BEGIN NETLIST
        SIGNAL "Result(0)"
        SIGNAL "Result(1)"
        SIGNAL "Result(2)"
        SIGNAL "Result(3)"
        SIGNAL "Result(4)"
        SIGNAL "Result(5)"
        SIGNAL "Result(6)"
        SIGNAL "Result(7)"
        SIGNAL "Result(8)"
        SIGNAL "Result(9)"
        SIGNAL "Result(10)"
        SIGNAL "Result(11)"
        SIGNAL "Result(12)"
        SIGNAL "Result(13)"
        SIGNAL "Result(14)"
        SIGNAL "Result(15)"
        SIGNAL "Result(15:0)"
        SIGNAL "zero"
        PORT Input "Result(15:0)"
        PORT Output "zero"
        BEGIN BLOCKDEF "or16"
            TIMESTAMP 2001 2 2 12 53 52
            LINE N 0 -448 48 -448 
            LINE N 48 -592 48 -1024 
            ARC N 28 -592 204 -416 192 -544 112 -592 
            LINE N 112 -496 48 -496 
            ARC N 28 -672 204 -496 112 -496 192 -544 
            LINE N 112 -592 48 -592 
            ARC N -40 -600 72 -488 48 -496 48 -592 
            LINE N 48 -64 48 -496 
            LINE N 256 -544 192 -544 
            LINE N 0 -640 48 -640 
            LINE N 0 -576 64 -576 
            LINE N 0 -512 64 -512 
            LINE N 0 -384 48 -384 
            LINE N 0 -320 48 -320 
            LINE N 0 -256 48 -256 
            LINE N 0 -192 48 -192 
            LINE N 0 -1024 48 -1024 
            LINE N 0 -960 48 -960 
            LINE N 0 -896 48 -896 
            LINE N 0 -832 48 -832 
            LINE N 0 -768 48 -768 
            LINE N 0 -704 48 -704 
            LINE N 0 -128 48 -128 
            LINE N 0 -64 48 -64 
        END BLOCKDEF
        BEGIN BLOCK "XLXI_1" "or16"
            PIN "I0" "Result(15)"
            PIN "I1" "Result(14)"
            PIN "I10" "Result(5)"
            PIN "I11" "Result(4)"
            PIN "I12" "Result(3)"
            PIN "I13" "Result(2)"
            PIN "I14" "Result(1)"
            PIN "I15" "Result(0)"
            PIN "I2" "Result(13)"
            PIN "I3" "Result(12)"
            PIN "I4" "Result(11)"
            PIN "I5" "Result(10)"
            PIN "I6" "Result(9)"
            PIN "I7" "Result(8)"
            PIN "I8" "Result(7)"
            PIN "I9" "Result(6)"
            PIN "O" "zero"
        END BLOCK
    END NETLIST
    BEGIN SHEET 1 3520 2720
        INSTANCE "XLXI_1" 1072 1280 R0
        BEGIN BRANCH "Result(0)"
            WIRE 1040 256 1072 256
            BEGIN DISPLAY 1040 256 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Result(1)"
            WIRE 1040 320 1072 320
            BEGIN DISPLAY 1040 320 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Result(2)"
            WIRE 1040 384 1072 384
            BEGIN DISPLAY 1040 384 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Result(3)"
            WIRE 1040 448 1072 448
            BEGIN DISPLAY 1040 448 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Result(4)"
            WIRE 1040 512 1072 512
            BEGIN DISPLAY 1040 512 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Result(5)"
            WIRE 1040 576 1072 576
            BEGIN DISPLAY 1040 576 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Result(6)"
            WIRE 1040 640 1072 640
            BEGIN DISPLAY 1040 640 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Result(7)"
            WIRE 1040 704 1072 704
            BEGIN DISPLAY 1040 704 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Result(8)"
            WIRE 1040 768 1072 768
            BEGIN DISPLAY 1040 768 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Result(9)"
            WIRE 1040 832 1072 832
            BEGIN DISPLAY 1040 832 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Result(10)"
            WIRE 1040 896 1072 896
            BEGIN DISPLAY 1040 896 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Result(11)"
            WIRE 1040 960 1072 960
            BEGIN DISPLAY 1040 960 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Result(12)"
            WIRE 1040 1024 1072 1024
            BEGIN DISPLAY 1040 1024 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Result(13)"
            WIRE 1040 1088 1072 1088
            BEGIN DISPLAY 1040 1088 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Result(14)"
            WIRE 1040 1152 1072 1152
            BEGIN DISPLAY 1040 1152 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Result(15)"
            WIRE 1040 1216 1072 1216
            BEGIN DISPLAY 1040 1216 ATTR "Name"
                ALIGNMENT SOFT-RIGHT
            END DISPLAY
        END BRANCH
        BEGIN BRANCH "Result(15:0)"
            WIRE 480 320 560 320
        END BRANCH
        IOMARKER 480 320 "Result(15:0)" R180 28
        BEGIN BRANCH "zero"
            WIRE 480 480 560 480
        END BRANCH
        IOMARKER 560 480 "zero" R0 28
        BEGIN BRANCH "zero"
            WIRE 1328 736 1360 736
            BEGIN DISPLAY 1360 736 ATTR "Name"
                ALIGNMENT SOFT-LEFT
            END DISPLAY
        END BRANCH
    END SHEET
END SCHEMATIC
